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Request For Proposals 
2022 City of Louisville Open Space Retaining Wall Replacement 
The City of Louisville is requesting proposals for the removal and rebuild of three sections of landscape timber retaining walls at the Dillion road underpass located across from the Coal Creek Golf Course in Louisville Colorado/The Grill at Coal Creek Golf Course https://goo.gl/maps/7ygnLL1ZrF9xbzUz9 (link to site location). The project will be to replace the sites retaining walls that were damaged in the Marshall Fire. Please see attached maps for more details and directions  

Cost estimates must be completed and submitted to npotopchuk@louisvilleco.gov by Wednesday, April 20, 2022 by 5:00pm.
	  1.
	Company Name:
	

	2.
	Company Contact Person Name:
	

	3.
	Company Contact Information:
	

	Address:
	

	
	

	Email:
	

	Phone:  
	

	Fax:
	


	
	

	Available Start Date:
	
	

	Completion Date:
	
	


	

Lump Sum Project Cost:
	$
	


	Contractor Recommendations:  
	

	


The project will include:

1. The demolition, removal, and disposal of all old retaining wall materials. Following  the provided design drawing located on page 6 of this document. The contractor selected by the City will install the new timber retaining wall. The retaining wall will have deadmen/anchor timbers every 8' for any area 3 tiers or higher. Deadmen/anchor timbers are to be anchored with concrete and rebar. Installation of 3/4” mountain granite drain rock or crushed rock gravel behind wall to alleviate pressure and assist with drainage. The rebuild shall be to City specification for the new retaining wall installation. Contractors are also responsible for restoring the site back to its existing status after the retaining wall work is completed. All disturbed vegetation will require top soil, reseeding, then covered with biodegradable erosion control blanketing (no plastics allowed). Any damage caused by the contractor shall be repaired at the contractor’s expense.
Scope of Work:
1. Contractor shall verify the location of existing underground utilities before the commencement of construction.  Should the contractor discover any conflicts while locating the existing utilities the owner’s representative must be notified immediately. The contractor must contact the Utility Notification Center of Colorado (UNCC) to complete this task. 

2. Contractor will be required to secure a Building Permit and Right of Way from the City of Louisville Planning Department. 

3. Contractor is responsible for obtaining tax exemption from the Colorado Department of Revenue if tax exemption is desired. 

4. Work is not permitted Friday through Sundays.

5. Contractors will keep open communication with Open Space Maintenance Tech III, Nick Potopchuk via email or phone for any questions, scheduling, and site assessment times. 

6. Contractor is responsible for scene safety, signage, closures, and for repairing any damage caused to vegetation or property.  Damage shall be repaired at the contractor’s expense.

7. Contractors are also responsible for restoring the site back to its existing status after the retaining wall work is completed, such as but not limited to: Seeding, Trail Repair, Sidewalk cleaning, etc. 
8. Contractor will obtain and use the short grass seed mix provided in this document to perform any site restorations and re-seeding.

9. Disturbed area will be layered with top soil and reseeded then covered with a biodegradable erosion control blanketing (No plastics allowed).

10. Contractors are responsible for the demolition and removal of the existing timber wall.

11. Contractors are responsible for the installation of the new timber wall.

Specs:

1. All lumber should be pressure treated to ACQ, CA, MCQ, or MCA standard. No CCA treated lumbers use is permitted. 

2. Contractor will use 6” x 6” x 8’ rough ground contact pressure treated landscape timbers following the standards presented in spec # 1. 

3. Contractor will stagger timbers such that each timber is approximately centered on the end of the timber in an adjacent row.

4. Install wood screws 6” from each end of timber.

5. Deadmen/anchor timbers are to be installed every 8' for any area 3 tiers or higher.

6. Contractors will use heavy duty 10" timberlok screws to secure the timbers to each other. 

7. Contractors will use ½” rebar to secure base level, corner points and deadmen/anchor timbers.

8. Deadmen/Anchor timbers will be anchored with concrete and rebar.

9. ¾” Mountain granite drain rock is to be installed and compacted behind the timbers of the wall at a minimum width of 4” (See Drawing).

10. See design drawing on page # 6 for all other details. 

11. Contractor will use biodegradable erosion control blanketing (No plastics allowed).
12. Contractor will obtain and use the short grass seed mix provided in this document to perform any site restorations and re-seeding
*Please note that all interested contractors must present proof of insurance with:  Workers' Compensation insurance, General Liability insurance with minimum combined single limits of ONE MILLION DOLLARS ($1,000,000) each occurrence and TWO MILLION DOLLARS ($2,000,000) aggregate, Comprehensive Automobile Liability insurance with minimum combined single limits for bodily injury and property damage of not less than FOUR HUNDRED THOUSAND DOLLARS ($400,000) per person in any one occurrence and ONE MILLION DOLLARS ($1,000,000) for two or more persons in any one occurrence, and auto property damage insurance of at least FIFTY THOUSAND DOLLARS ($50,000) per occurrence.
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Site Access Map:
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Design Drawings:
Seed Mix:
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CERTIFICATION OF COMPLIANCE

SOLD BY: ARKANSAS VALLEY SEED

4300 MONACO STREET
DENVER, CO 80216

SOLD TO: GOODLAND CONSTRUCTION

JOB NAME: MCCASLIN BOULEVARD- SEED MIX B

STATEMENT

WE HEREBY CERTIFY THAT THE MATERIAL FURNISHED AND DESCRIBED
'BELOW, DO MEET OR EXCEED THE CURRENT COLORADO STATE SEED LAW
SPECIFICATIONS.

MATERIAL SUPPLIED

% Or Plstiac DESCRIPTION 'MANUFACTURED BY
2.0pls# | Sideoats Grams, Vaughn ‘Arkansas Valley Seed
33pls# | Buffalograss, Cod “Atkansas Valley Seed
L0pls# | Sandberg Bluegrass, Canbar | Arkansas Valley Seed
0.7pls# | Prairie Junegrass ‘Arkansas Valley Sced
3.3pls#_| Bluc Grama, Nagive “Arkansas Valley Seed

|
|

PLIER REPRESENTATIVE
PAULF. APODACA
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